 


Directions on the X-8500_040615_230_api.bin


In the 2500a receiver satellite directory you should find the factroy default setting. Click on this to restore your receiver to factory default.


Next up load the X-8500_040615_230_api. listed on the dsscentralFTA page.


Set your pansat receiver to the dishnetwork 119 satellite , click on the ECHO 7 satellite, set the LNB to 11250, set the 22khz to on (if your using a 3 lnb dish) scroll to the TP setting and right click till the TP goes to 13 at this time you should have a good quality reading (over 70%) if not reaim your dish.


CLick exit then ok to save and exit again to go to menu, find the blind scan and click on it and let it go. It will blind scan and automatically go into the satellite scan mode.  After scanning go to the Parental Control setting in menu, enter password 0000 and go to keycode and right click to ON setting. When done you should get the Network channels in different cities unscrambled.  THIS  IS THE BEST I HAVE FOUND ON THE 119 DISH SATELLITE....


Can't wait till the fix for 8/12 comes!











